Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Remove the Front I/O Board

1. Prepare the server for service. See How to Prepare the Server for Service.
2. Remove all fan trays from the fan tray carriage. See How to Remove the Fan Tray.
3. Remove all CPU modules or CPU filler boards from the chassis. See How to Remove a CPU Module or Filler Card.
4. Remove the fan tray carriage from the chassis. See How to Remove the Fan Tray Carriage.
5. Disconnect the two flex cable connectors that come from the front panel indicator board from the front I/O board and the motherboard.

   It is not necessary to remove the front panel indicator board.

6. Remove the two screws that secure the front I/O board to the chassis floor.
7. Remove the board from the chassis.

See Also

- How to Install the Front I/O Board

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |