Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Linux Installation Guide Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Install Portmap on Your DHCP Server

If your server does not include a portmap server, you need to install it.

1. Determine whether the portmap server package is already installed on the server. Type:

       # rpm -qa | grep portmap

2. If portmap is not listed, install it as follows:
   1. Mount the CD/DVD drive.

          # mount /dev/cdrom /mnt/cdrom

   2. Install the portmap server.
      - For RHEL 4.8, insert the DVD or CD2 and type:

            # rpm -Uvh /mnt/cdrom/RedHat/RPMS/portmap-*

      - For RHEL 5.3, insert the DVD or CD1 and type:

            # rpm -Uvh /mnt/cdrom/Server/portmap-*

      - For SLES10 SP2, insert DVD1 or CD1 and type:

            # rpm -Uvh /mnt/cdrom/suse/x86_64/portmap*

      - For SLES11, insert DVD1 and type:

            # rpm -Uvh /mnt/cdrom/suse/x86_64/portmap*

   3. Unmount the CD/DVD drive. Type:

          # umount /dev/cdrom /mnt/cdrom

   4. Remove the CD or DVD from the CD/DVD drive.

Next Steps

How to Configure the TFTP Service on Your DHCP Server

Copyright © 2009, 2010, Oracle and/or its affiliates. All rights reserved. Legal Notices |