Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Install a Power Supply

1. Align the power supply with the empty bay in the chassis.
2. Slide the power supply into the bay until it firmly engages the connector on the power distribution board, indicated when the thumb latch on the power supply clicks into place.
3. Connect the AC power cord to the new power supply.
4. If necessary, prepare the server for operation. See How to Prepare the Server for Operation.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |