Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

##### Power Specifications For the Sun Fire X4640 Server

Specification | Value
--- | ---
Universal AC input | 110 – 240 VAC 50/60 Hz
Maximum input current at 200 VAC | 13 A
Maximum input current at 100 VAC | 22 A
Maximum power available | 1975 W
Maximum power consumed | 1715 W

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |