Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

##### Cabling Diagram

Table 1 Cabling Diagram

Figure Legend
1 | Connect power cable to power source.
2 | Connect a serial cable between the SER MGT port and a terminal device or a PC. Note - You might need an adapter. The server comes with a DB9–to-RJ45 serial port adapter.
3 | (Optional) Connect an Ethernet cable between the NET MGT port and the network to which future connections to the SP and the host will be made.
4 | Connect an Ethernet cable between one of the NET ports and the network.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |