Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Notes Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## Integrated Lights Out Manager (ILOM) Issues

Note - Fixed issues appear at the bottom of the table.

ILOM Issues | Workaround
--- | ---
Service Processor Does Not Log Event or Provide Visual Alert After Hard Disk Is Removed | No
Recovery for Accidentally Flashing the Wrong Platform Firmware on the Sun Fire X4640 Server | No
Unimplemented Simple Network Management Protocol (SNMP) Traps (6300437) | No
SNMP Agent Does Not Handle All Sets (6255301) | Yes
(Fixed in SW 1.1) FRU List Is Not Updated When Power Supply Is Hot-Swapped (6894442) | Yes

For a documentation issue related to ILOM, see ILOM Supplement Missing How to Prove Physical Presence (6881237).

Copyright © 2009, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |