Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Product Documentation Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

##### Slide Rail Kit

The slide rail kit that comes with your server is called the express slide rail or the tool-less slide rail because it is simpler than older slide rails. It can be used with both square-hole and round-hole racks. The cable management arm (CMA) might come in a separate box.

Figure Legend
1 | Slide rail (2) | Attaches to rack post. The slide rail has an outer rail and a middle section. The middle section has the ball bearings which slide forward and backward. Each end of the slide rail has an attachment assembly.
2 | Mounting bracket (2) | Attaches to server. The mounting bracket is also called the inner section because it is inserted into the middle section of the slide rail.
3 | (Optional) Cable management arm (CMA) | Included only with Express Slide Rail and CMA combination kit.
4 | Shipping/hardmount hardware | Note - If you want to secure the server for shipping now or in the future, use the shipping hardware. It is not possible to install the shipping hardware after the slide rails are installed. It is better to install the shipping hardware during the slide rail installation.

The slide rail kit comes with the following shipping hardware:

Figure Legend
1 | M6 screws (9) | To secure server for shipping, install 8 screws, 2 per rack post. One extra screw is supplied.
2 | Cage nuts | Cage nuts are required for shipping server in square-hole racks.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |