Skip Navigation Links
Exit Print View
| Sun ILOM 3.0 Supplement for the Sun Fire X4640 Server Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Connect to the ILOM Web Interface

Before You Begin

- Perform the hardware setup as described in the hardware setup documentation.

- Apply standby power to the server by connecting AC power to the system power supply. See Server Connections for the location of the power connectors.

1. Type the IP address of the ILOM SP in the browser locator box and press Enter.

   For example, if the IP address for your ILOM SP is 129.144.02.20, you would enter it as shown here:

2. Log in to the web interface using the default user name, `root`, and the default password, `changeme`.

Copyright © 2009, 2010, Oracle and/or its affiliates. All rights reserved. Legal Notices |