Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Remove a PCI Card

1. Prepare the server for service. See How to Prepare the Server for Service.
2. Working from the rear of the chassis, push the handle of the locking lever slightly downward and then pivot both PCI slot locking levers upward to release the card.
3. Pull the PCI card up and out of the PCI slots.
4. Pivot the PCI card latches back to their closed positions.
5. If necessary, prepare the server for operation. See How to Prepare the Server for Operation.

See Also

- How to Install a PCI Card

- Identifying Components

- PCI Slot Designations

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |