Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Service Manual Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

## How to Remove the Front Bezel

1. Hold the bezel at both side edges.
2. Pull the bezel away from the chassis, being careful to evenly release all seven pegs on the bezel from the chassis.

   Note - Avoid bending the bezel by gradually pulling it from the middle and both ends simultaneously.

See Also

- How to Prepare the Server for Service

- How to Install the Front Bezel

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |