Skip Navigation Links
Exit Print View
| Sun Fire X4640 Server Installation Guide Sun Fire X4640 Server Documentation Library

Search Scope:

- This Document
- Entire Library

### Determining the SP IP Address

You need to determine the service processor (SP) IP (network) address to use the SP Integrated Lights Out Manager (ILOM) to manage the server.

You can determine the IP address through either one of these ways:

- How to Get the SP IP Address Using the BIOS Setup Utility

- How to Get the SP IP Address By Using a Serial Connection and the CLI

Copyright © 2009, 2010, Oracle and/or its affiliates. All rights reserved. Legal Notices |