Sun Java System Application Server Enterprise Edition 8.1 2005Q2 Performance Tuning Guide

- Previous: Virtual Memory
- Next: Disk I/O Settings

## Network Interface

To ensure that the network interface is operating in full duplex mode, add the following entry into `/etc/rc.local`:

    mii-tool -F 100baseTx-FD eth0

where eth0 is the name of the network interface card (NIC).

- Previous: Virtual Memory
- Next: Disk I/O Settings

- © 2010, Oracle Corporation and/or its affiliates