Sun Java System Application Server Enterprise Edition 8.1 2005Q2 Deployment Planning Guide

- Previous: Using Clusters to Improve Availability
- Next: Using HADB Redundancy Units to Improve Availability

### Identifying Failure Classes

The level of redundancy is determined by the failure classes (types of failure) that the system needs to tolerate. Some examples of failure classes are:

- System process

- Machine

- Power supply

- Disk

- Network failures

- Building fires or other preventable disasters

- Unpredictable natural catastrophes

Duplicated system processes tolerate single system process failures, as well as single machine failures. Attaching the duplicated mirrored (paired) machines to different power supplies tolerates single power failures. By keeping the mirrored machines in separate buildings, a single-building fire can be tolerated. By keeping them in separate geographical locations, natural catastrophes like earthquakes can be tolerated.

- Previous: Using Clusters to Improve Availability
- Next: Using HADB Redundancy Units to Improve Availability

- © 2010, Oracle Corporation and/or its affiliates