Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## C.5 Video Connectors

There are two video connectors (VGA) one on the front and one on the back of the server.

Figure C-5 Video Connector

Figure Legend

1 Red Video

2 Green Video

3 Blue Video

4 Monitor ID - Bit 2 (Ground)

5 Ground

6 Red Ground

7 Green Ground

8 Blue Ground

9 +5V

10 Sync Ground

11 Monitor ID - Bit 0 (Ground)

12 VGA 12C Serial Data

13 Horizontal Sync

14 Vertical Sync

15 VGA 12C Serial Clock

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |