Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## 2.8 Removing or Installing Filler Panels

Each server is shipped with module-replacement filler panels for CPUs, disk drives (HDD or SSD), memory modules (DIMMs), the DVD drive, and the PCIe cards. A filler panel is an empty metal or plastic enclosure that does not contain any functioning system hardware or cable connectors.

The filler panels are installed at the factory and must remain in the server until you replace them with a purchased module to ensure proper airflow through the system. If you remove a filler panel and continue to operate your system with an empty module slot, the server might overheat due to improper airflow. For instructions on removing or installing a filler panel for a server component, refer to the section in this guide about servicing that component.

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |