Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server ### Service Manual

Search Scope:

- This Document
- Entire Library

## 2.5 Releasing the Cable Management Arm

For some service procedures, if you are using a cable management arm (CMA), you might have to release the CMA to gain access to the back of the chassis.

## Release the CMA

Refer to Releasing the Cable Management Arm for the following procedure.

1. Press and hold the tab [1].
2. Swing the CMA out of the way [2].

   When you have finished with the service procedure, swing the CMA closed and latch it to the left rack rail.

   Figure 2-3 Releasing the Cable Management Arm

Copyright © 2010, 2011 , Oracle and/or its affiliates. All rights reserved. Legal Notices |