Skip Navigation Links
Exit Print View
| Sun Fire X4470 Server Installation Guide

Search Scope:

- This Document
- Entire Library

### Disassembling Slide-Rails

Complete the following procedures to disassemble the slide-rails before installation.

# Disassemble Slide-Rails

To remove the mounting brackets from the slide-rail assemblies:

1. Unpack the slide-rails.
2. Locate the slide-rail lock at the front of one of the slide-rail assemblies (Disassembling the Slide-Rail Before Installation).
3. Press and hold the slide-rail lock toward the direction of the arrow, while you pull the mounting bracket out of the slide-rail assembly until it reaches the stop (Disassembling the Slide-Rail Before Installation).
4. Push the mounting bracket release button toward the front of the mounting bracket (Disassembling the Slide-Rail Before Installation), and simultaneously withdraw the mounting bracket from the slide-rail assembly.
5. Repeat for the remaining slide-rail assembly.

   Figure 2-1 Disassembling the Slide-Rail Before Installation

   Figure Legend

   1 Slide-rail lock

   2 Mounting bracket release button

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |