Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Server Overview

The server is a rack-mountable system with a 2RU form-factor.

Figure 2 SPARC T3-1 Server

The following list identifies the items that comprise the server's base configuration:

- 2 RU system enclosure with rack-mount slide hardware.

- Motherboard with a service processor, two embedded RAID 0, 1, and 1E hard drive controllers, system configuration PROM, and other system infrastructure components.

- Memory slots for up to sixteen DDR3 memory modules.

- A hard drive enclosure with 8 or 16 drive bays and a corresponding connector backplane that can support either 8 or 16 hard disk drives (HDDs).

- An optical disk drive that fits into the hard drive enclosure and plugs into the disk backplane.

- Six fan modules (two fans per module).

- One or two power supplies and associated power distrubution circuitry.

- I/O interface assembly to support up to six PCIe expansion modules. Two slots may be used by XAUI modules.

##### Related Information

- Front Panel Components

- Front Panel System LEDs and Buttons

- Rear Panel Components

- Rear Panel System LEDs and Button

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |