Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the DVD/USB Assembly

Note - This is a cold service procedure that can be performed by customers. See Cold Service, Replaceable by Customer for more information about cold service procedures.

| Caution - Be certain the DVD module you will install is of the serial ATA (SATA) type.

1. Perform the preliminary steps required for cold service procedures.

   See Cold Service, Replaceable by Customer for instructions.

2. Slide the DVD/USB module into the front of the chassis until it seats.
3. Slide the release tab back into the system.
4. If you removed a hard drive from the lower right drive bay, reinstall it.
5. Plug in the power cords.

   See Reconnect the Power Cords.

6. Power on the system.

   See Power On the Server (`start /SYS` Command) or Power On the Server (Power Button).

##### Related Information

- Remove the DVD/USB Assembly

- DVD/USB Assembly Overview

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |