Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Disk Zone Status (`probe-scsi-all`)

The following `probe-scsi-all` output examples show the difference in how storage devices are listed when zoning is enabled and when it is disabled. There are 10 disks represented in both examples. They are identified as PhyNum 0-9.

Note - The entries for PhyNum 1-6 are omitted in these examples to reduce the size of the examples. The missing entries would not alter the illustration of the concept.

Zoning is disabled:

When zoning is disabled, each disk is visible to both controllers. The following example shows this by listing every disk with controller 0 and with controller 1.

Tip - Note that SASDeviceName and SASAddress for each PhyNum listed under controller 1 matches the corresponding PhyNum’s DeviceName and SASAddress listed under controller 0. This is true for PhyNum 1-6, which were omitted to reduce the size of the table.

    {0} ok probe-scsi-all
    /pci@400/pci@2/pci@0/pci@f/pci@0/usb@0,2/hub@2/hub@3/storage@2
      Unit 0   Removable Read Only device    AMI     Virtual CDROM   1.00

    /pci@400/pci@2/pci@0/pci@4/scsi@0                          <==== Controller 1

    FCode Version 1.00.56, MPT Version 2.00, Firmware Version 5.00.13.00

    Target a
      Unit 0   Removable Read Only device   TEAC    DV-W28SS-R      1.0C
      SATA device  PhyNum 6
    Target b
      Unit 0   Disk   SEAGATE  ST930003SSUN300G 0868    585937500 Blocks, 300 GB
      SASDeviceName 5000c50017b0c14b  SASAddress 5000c50017b0c149  PhyNum 0

             [PhyNum 1-6 are omitted to conserve space.]

    Target 12
      Unit 0   Disk   SEAGATE  ST973402SSUN72G  0400    143374738 Blocks, 73 GB
      SASDeviceName 5000c50003d5c6a3  SASAddress 5000c50003d5c6a1  PhyNum 7
    Target 13
      Unit 0   Disk   SEAGATE  ST914603SSUN146G 0768    286739329 Blocks, 146 GB
      SASDeviceName 5000c50012ef2247  SASAddress 5000c50012ef2245  PhyNum 8
    Target 14
      Unit 0   Disk   SEAGATE  ST973402SSUN72G  0400    143374738 Blocks, 73 GB
      SASDeviceName 5000c50003d49c77  SASAddress 5000c50003d49c75  PhyNum 9
    Target 15
      Unit 0   Encl Serv device   SUN      SAS2 X16DBP      0302
      SASAddress 500605b0000272bd  PhyNum 18

    /pci@400/pci@1/pci@0/pci@4/scsi@0                          <==== Controller 0

    FCode Version 1.00.56, MPT Version 2.00, Firmware Version 5.00.13.00

    Target a
      Unit 0   Disk   SEAGATE  ST930003SSUN300G 0868    585937500 Blocks, 300 GB
      SASDeviceName 5000c50017b0c14b  SASAddress 5000c50017b0c149  PhyNum 0

             [PhyNum 1-6 are omitted to conserve space.]

    Target 11
      Unit 0   Disk   SEAGATE  ST973402SSUN72G  0400    143374738 Blocks, 73 GB
      SASDeviceName 5000c50003d5c6a3  SASAddress 5000c50003d5c6a1  PhyNum 7
    Target 12
      Unit 0   Disk   SEAGATE  ST914603SSUN146G 0768    286739329 Blocks, 146 GB
      SASDeviceName 5000c50012ef2247  SASAddress 5000c50012ef2245  PhyNum 8
    Target 13
      Unit 0   Disk   SEAGATE  ST973402SSUN72G  0400    143374738 Blocks, 73 GB
      SASDeviceName 5000c50003d49c77  SASAddress 5000c50003d49c75  PhyNum 9
    Target 14
      Unit 0   Encl Serv device   SUN      SAS2 X16DBP      0302
      SASAddress 500605b0000272bd  PhyNum 18

    {0} ok

Zoning is enabled:

In the following example, zoning is enabled and each disk is shown connected to a single SAS-2 controller. PhyNum 0-7 are connected to controller 0 and PhyNum 8-9 are connected to controller 1``.

    {0} ok probe-scsi-all
    /pci@400/pci@2/pci@0/pci@f/pci@0/usb@0,2/hub@2/hub@3/storage@2
      Unit 0   Removable Read Only device    AMI     Virtual CDROM   1.00

    /pci@400/pci@2/pci@0/pci@4/scsi@0                          <==== Controller 1

    FCode Version 1.00.56, MPT Version 2.00, Firmware Version 5.00.13.00

    Target a
      Unit 0   Disk   SEAGATE  ST914603SSUN146G 0768    286739329 Blocks, 146 GB
      SASDeviceName 5000c50012ef2247  SASAddress 5000c50012ef2245  PhyNum 8
    Target b
      Unit 0   Disk   SEAGATE  ST973402SSUN72G  0400    143374738 Blocks, 73 GB
      SASDeviceName 5000c50003d49c77  SASAddress 5000c50003d49c75  PhyNum 9
    Target c
      Unit 0   Encl Serv device   SUN      SAS2 X16DBP      0305
      SASAddress 50800200000272bd  PhyNum 18
    Target d
      Unit 0   Removable Read Only device   TEAC    DV-W28SS-R      1.0C
      SATA device  PhyNum 6

    /pci@400/pci@1/pci@0/pci@4/scsi@0                          <==== Controller 0

    Target a
      Unit 0   Disk   SEAGATE  ST930003SSUN300G 0868    585937500 Blocks, 300 GB
      SASDeviceName 5000c50017b0c14b  SASAddress 5000c50017b0c149  PhyNum 0

             [PhyNum 1-6 are omitted to conserve space.]

    Target 11
      Unit 0   Disk   SEAGATE  ST973402SSUN72G  0400    143374738 Blocks, 73 GB
      SASDeviceName 5000c50003d5c6a3  SASAddress 5000c50003d5c6a1  PhyNum 7
    Target 12
      Unit 0   Encl Serv device   SUN      SAS2 X16DBP      0305
      SASAddress 50800200000272bd  PhyNum 18

    {0} ok

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |