Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Cold Service, Replaceable by Authorized Service Personnel

The following table identifies components that must be replaced by authorized service personnel. These replacement procedures can only be done when the server is powered down and power cables are unplugged.

Authorized Service Personnel Only - Cold Service (power down system and disconnect power cables) | Notes
--- | ---
Motherboard | Transfer System Configuration PROM to new motherboard.
Fan power board |
Power Distribution Board (PDB) | Configure new PDB with the chassis serial and part numbers.
Power supply backplane |
Connector board |
Hard Drive backplane | This requires removal of the Hard Drive cage first.
Light pipe assembly | This requires removal of the Hard Drive cage first.

See Cold Service, Replaceable by Customer for the steps involved in shutting down the server.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |