Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect the SER MGT Port Cable

Before You Begin

The service processor serial management port is marked SER MGT. This port is the farthest left RJ-45 port on the rear panel.

- Connect a Category 5 cable from the SER MGT serial management port to the terminal device.

  Figure 30 Service Processor Serial Management Port – Rear Panel

  This port is needed to set up the service processor network management port.

  When connecting a DB-9 cable, use an RJ-45 to DB-9 adapter to perform the crossovers given for each connector.

  Note - Use the service processor serial management port only for server management. This port is the default connection between the service processor and a terminal or a computer.

  | Caution - Do not attach a modem to this port.

##### Related Information

- Connect the NET MGT Port Cable

- Connecting the Server Cables

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |