Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Display System Components

The `show components` command displays the system components (`asrkeys`) and reports their status.

- At the Oracle ILOM prompt, type `show components`.

  In the following example, PCIE3 is shown as disabled.

      -> show components
      Target              | Property               | Value
      --------------------+------------------------+-------------------------------
      /SYS/MB/RISER0/     | component_state        | Enabled
      PCIE0               |                        |
      /SYS/MB/RISER0/     | component_state        | Disabled
      PCIE3               |                        |
      /SYS/MB/RISER1/     | component_state        | Enabled
      PCIE1               |                        |
      /SYS/MB/RISER1/     | component_state        | Enabled
      PCIE4               |                        |
      /SYS/MB/RISER2/     | component_state        | Enabled
      PCIE2               |                        |
      /SYS/MB/RISER2/     | component_state        | Enabled
      PCIE5               |                        |
      /SYS/MB/NET0        | component_state        | Enabled
      /SYS/MB/NET1        | component_state        | Enabled
      /SYS/MB/NET2        | component_state        | Enabled
      /SYS/MB/NET3        | component_state        | Enabled
      /SYS/MB/PCIE        | component_state        | Enabled

##### Related Information

- ASR Overview

- Disable System Components

- Enable System Components

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |