Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Manage the Host Boot Mode Script

- At the Oracle ILOM`->` prompt, type:

      -> set /HOST/bootmode script=value

  where `script` controls the host server OpenBoot PROM firmware method of booting.

  `script` does not affect the current `/HOST/bootmode` setting.

  value can be up to 64 bytes in length.

  You can specify a `/HOST/bootmode` setting and set the script within the same command. For example:

      -> set /HOST/bootmode state=reset_nvram script="setenv diag-switch? true"

  After the server resets and OpenBoot PROM reads the values stored in the script, the OpenBoot PROM sets the OpenBoot PROM variable `diag-switch?` to the user-requested value of `true`.

  Note - If you set `/HOST/bootmode script=""`, Oracle ILOM sets the `script` to empty.

##### Related Information

- Reset the Server From Oracle ILOM

- Boot Mode Overview

- Oracle VM Server for SPARC Overview

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |