Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove the Top Cover

1. Unlatch the fan module door.

   Pull the release tabs back to release the door.

2. Press the top cover release button and slide the top cover to the rear about a 0.5 inch (12.7 mm).
3. Remove the top cover.

   Lift up and remove the cover.

##### Related Information

- Install the Top Cover

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |