Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Identify Faulty DIMMs Using the `show faulty` Command

The Oracle ILOM `show faulty` command displays current system faults, including DIMM failures.

- Enter `show faulty` at the `->` prompt.

      -> show faulty
      Target              | Property               | Value
      --------------------+------------------------+-------------------------------
      /SP/faultmgmt/0     | fru                    | /SYS/MB/CMP0/B0B0/CH0/D0
      /SP/faultmgmt/0     | timestamp              | Dec 21 16:40:56
      /SP/faultmgmt/0/    | timestamp              | Dec 21 16:40:56 faults/0
      /SP/faultmgmt/0/    | sp_detected_fault      | /SYS/MB/CMP0/B0B0/CH0/D0
      faults/0            |                        | Forced fail(POST)

##### Related Information

- Remove a DIMM

- Install a DIMM

- Verify DIMM Functionality

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |