Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### WWN Syntax in an OS Installation on a RAID Volume

The following Oracle Solaris Jumpstart profile example shows how to use the WWN syntax when installing the OS on a RAID volume. When installing software on a RAID volume, use the virtual device’s `VolumeDeviceName` instead of an individual device name. In this example, the RAID volume name is `3ce534e42c02a3c0`.

    #
    install_type flash_install
    boot_device 3ce534e42c02a3c0     preserve

    archive_location nfs 129.148.94.249:/export/install/media/solaris/builds/s10u9/flar/latest.flar

    # Disk layouts
    #
    partitioning explicit
    filesys rootdisk.s0         free /
    filesys rootdisk.s1         8192 swap

##### Related Information

- World Wide Name Syntax

- `probe-scsi-all` Output Example (SPARC T3-1, Eight-Disk Backplane)

- `probe-scsi-all` Output Example (SPARC T3-1, Sixteen-Disk Backplane)

- `probe-scsi-all` Output Example (SPARC T3-4)

- Identify a Disk Slot Using `probe-scsi-all` (OBP)

- Identify a Disk Slot Using `prtconf` (Oracle Solaris, Onboard Controllers)

- Identify a Disk Slot Using `prtconf` (Oracle Solaris, Single Initiator)

- WWN Syntax in an OS Installation on a Specific Device

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |