Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### POST-Detected Fault Example (`show` `faulty` Command)

The following is an example of the `show` `faulty` command displaying a fault that was detected by POST. These kinds of faults are identified by the message `Forced` `fail` reason, where reason is the name of the power-on routine that detected the fault.

    -> show faulty
    Target              | Property               | Value
    --------------------+------------------------+--------------------------------
    /SP/faultmgmt/0     | fru                    | /SYS/PM0/CMP0/B0B0/CH0/D0
    /SP/faultmgmt/0     | timestamp              | Oct 12 16:40:56
    /SP/faultmgmt/0/    | timestamp              | Oct 12 16:40:56
    faults/0            |                        |
    /SP/faultmgmt/0/    | sp_detected_fault      | /SYS/PM0/CMP0/B0B0/CH0/D0
    faults/0            |                        | Forced fail(POST)

##### Related Information

- Fault Managment Command Examples

- `show` `faulty` Example of a Power Supply Fault

- `fmadm` `faulty` Example of a Power Supply Fault

- `show` `faulty` Example of a PSH-Detected Fault

- Service-Related Oracle ILOM Command Summary

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |