Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Initial Power-On Tasks Overview

When you power on the server for the first time, you must take various steps that are not required in subsequent power-on sessions.

Preparatory step | Purpose
--- | ---
Connect a terminal or terminal emulator to the SER MGT port. | This enables logging into the service processor before it has been configured for network access. Connect a Terminal or Emulator to the SER MGT Port
Log in to the service processor and change the default root password. | To protect the system from unauthorized superuser access, change the default password to a secure value. Power On the Server for the First Time
Start the Oracle ILOM system console. | This enables you to monitor system initialization output generated by the Oracle ILOM firmware. Power On the Server for the First Time
Configure the Oracle Solaris OS. | The preinstalled Oracle Solaris OS is shipped in the unconfigured state. Power On the Server for the First Time
(If necessary) Specify a static IP address. | DHCP is the default IP addressing protocol. If your server will be connected to a network that uses static IP addressing, you will need to assign a static IP address to the service processor. Assign a Static IP Address to the Service Processor

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |