Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

## Remove SLB-L2 Port Members

This example shows removing one port member from a SLB-L2 group. You use the same process to remove an active or standby port member.

1. Remove the member entry.

       SEFOS# configure terminal
       SEFOS(config)# no slb l2 1 extreme-ethernet 0/5
       SEFOS(config)# end

2. Show current LBGs and members.

   The following example shows the removal of one of the active SLB server members.

       SEFOS# show slb

       L2 SLB Group #1:
               Failover Method: Failover to All Ports
       Port Members:
       Port    State     Comments
       ====    =====     ==================
       3       ACTIVE
       4       ACTIVE
       6       STANDBY

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |