Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure RFC 1583 Compatibility

This procedure sets the OSPF compatibility list to be compatible with RFC 1583.

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf

2. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

3. Enable OSPF over the VLAN interface and associate the interface with an OSPF area.

       SEFOS(config-router)# network 10.4.0.1 area 0.0.0.0
       SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6

4. Configure RFC 1583 compatibility.

       SEFOS(config-router)# compatible rfc1583

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |