Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

#### SER MGT Port

A single RJ-45 serial management port provides CLI connections to a system console for administering the switch at the physical location.

This figure and table describe the pinouts of the SER MGT connector.

Pin | Signal
--- | ---
1 | RTS
2 | DTR
3 | TXD
4 | GND
5 | GND
6 | RXD
7 | DSR
8 | CTS

##### Related Information

- NET MGT Port

- Connect the SER MGT Cable

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |