Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Create a PIM Component

This example creates PIM component 2.

1. Create a PIM component.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim enable
       SEFOS(config)# ip pim component 2
       SEFOS(pim-comp)# end

2. Ensure that PIM component 2 was created.

       SEFOS# show ip pim component 2

       PIM Component Information
       ---------------------------
       Component-Id: 2
         PIM Mode: sparse,   PIM Version: 2
         Elected BSR: 0.0.0.0
         Candidate RP Holdtime: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |