Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable IPv6 Support and Assign IPv6 Addresses

1. Enable IPv6 support in the VLAN.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan vlan_id
       SEFOS(config-if)# ipv6 enable

2. Configure the IPv6 address in the interface.

       SEFOS(config-if)# ipv6 address ipv6_address mask
       SEFOS(config-if)# ipv6 address ipv6_address scope_of_the_ipv6_address

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |