Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Connect to SEFOS

1. Connect to the Oracle ILOM CLI.

   See Log Into Oracle ILOM CLI (SER MGT).

2. Access the SEFOS prompt.

   The `SEFOS#` prompt appears. For example:

       -> cd /SYS/fs_cli/
       cd: Connecting to Fabric Switch CLI as user root

       SEFOS#

   You can now configure SEFOS. Refer to the Sun Network 10GbE Switch 72p Software Configuration Guide for the Sun Ethernet Fabric Operating System for those instructions.

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |