Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the IPv6 Route Redistribution Policy for Routing Protocols

The RRD policy feature uses a routing protocol to advertise routes that are learned by other routing protocols. The routes can be static routes or directly connected routes. This procedure shows how to configure the policy set for routing IPv6 routes. The IPv6 routes are maintained in the RTM6 table that is used for IPV6 routes, ensuring that the route table manager redistributes the best route.

This procedure shows how to configure the IPv6 route redistribution policy for routing protocols:

- Configure the IPv6 Route Resitribution Policy for Routing Protocols

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |