C H A P T E R 20

UDP

UDP is a portable implementation of the industry-standard UDP. UDP is used in packet-switched computer communication networks and in interconnected systems of such networks. The software consists of the core UDP protocol and a library that provides a socket layer interface (similar to BSD sockets) for applications like SNMP. The SEFOS UDP module supports a number of standard features in addition to the core protocol.

##

20.1 UDP Commands

The following is the list of UDP commands:

- show udp statistics

- show udp connections

### 20.1.1 `show udp statistics`

Displays the `udp` statistics.

    show udp statistics

Mode | Privileged EXEC
Example | SEFOS# show udp statistics InDatagrams = 81032 OutDatagrams = 83311 HC InDatagrams = 81032 HC OutDatagrams = 83311 UDP No Ports = 2263 UDP In Errors = 0

#### Related Commands

- show udp connections - Displays the UDP connections

### 20.1.2 `show udp connections`

Displays the `udp` connections.

    show udp connections

Mode | Privileged EXEC
Example | SEFOS# show udp connections UDP Connections =============== Local IP Address Type : IPv4 Local IP : 0.0.0.0 Local Port : 631 Remote IP Address Type : IPv4 Remote IP : 0.0.0.0 Remote Port : 0 Local IP Address Type : IPv4 Local IP : 0.0.0.0 Local Port : 1013 Remote IP Address Type : IPv4 Remote IP : 0.0.0.0 Remote Port : 0 Local IP Address Type : IPv4 Local IP : 30.0.0.40 Local Port : 8001 Remote IP Address Type : IPv4 Remote IP : 0.0.0.0 Remote Port : 0

#### Related Commands

- show udp statistics - Displays the UDP statistics

Copyright © 2012, Oracle and/or its affiliates. All rights reserved.