Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Delete a PIM Interface

This example deletes the `VLAN 5` interface.

1. Enable PIM globally.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim enable

2. Enter Interface Configuration mode for the interface.

       SEFOS(config)# interface vlan 5

3. Delete the VLAN interface at the PIM level.

       SEFOS(config-if)# no ip pim interface
       SEFOS(config-if)# end

4. Ensure the correct PIM interface status has been set. For this example, `VLAN 5` must not appear.

       SEFOS(config-if)# show ip pim interface detail

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |