Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

#### Enabling a Specific Management Address

Management address TLV transmission status is disabled by default. If a management address is configured for the system or the existing management address is changed, the TLV transmission status of the management address is disabled by default.

These procedures show how to enable a specific management address:

- Enable a New IP Address

- Enable an Existing IP Interface

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |