Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable VLANs

You can enable a VLAN by adding a member port or by using the `vlan active` command. The following example shows VLAN 2 being enabled.

1. Configure VLAN 2 in the switch.

       SEFOS# configure terminal
       SEFOS(config)# vlan 2

2. Enable the VLAN.

       SEFOS(config-vlan)# vlan active

   Note - If the `vlan active` command is used without configuring the member ports, the VLAN will have zero member ports. Resources are allocated for active VLANs.

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |