Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

## Display Output of Unstarted DCBX Protocol Exchange

In the following output, all controls and features are zeroes, which indicates that the DCBX protocol exchange has not yet been started.

- Type.

      SEFOS# show interfaces extreme-ethernet 0/2 dcb counters

      Port                 :  Ex0/2
      Show Type            :  Control and Feature Stats
      Control Info Stats   :
        SeqNo              :  0
        AckNo              :  0
        Frames Out         :  0
        Frames In          :  0
      Priority Group       :
        Frames Out         :  0
        Frames In          :  0
      Priority Flow Control:
        Frames Out         :  0
        Frames In          :  0

      Application Proto    :
        Frames Out         :  0
        Frames In          :  0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |