Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable the Fast Leave Process

1. Enter the configuration mode for the VLAN interface.

       SEFOS# configure terminal

2. Disable the fast leave process for the VLAN.

       SEFOS(config-vlan)# no ip igmp snooping fast-leave

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |