Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

## Clear the Statistics for All VLANs

1. Enter Global Configuration mode.

       SEFOS# configure terminal

2. Clear the statistics for all of the VLANs.

       SEFOS(config)# ip igmp snooping clear counters
       SEFOS(config)# end

3. Review the statistics.

       SEFOS# show ip igmp snooping statistics

       Snooping Statistics for VLAN 1
         General queries received: 0
         Group specific queries received: 0
         Group and source specific queries received: 0
         ASM reports received: 0
         SSM reports received: 0
         IS_INCLUDE messages received: 0
         IS_EXCLUDE messages received: 0
         TO_INCLUDE messages received: 0
         TO_EXCLUDE messages received: 0
         ALLOW messages received: 0
         Block messages received: 0
         Leave messages received: 0
         General queries transmitted: 0
         Group specific queries transmitted: 0
         Group and source specific queries transmitted : 0
         ASM reports transmitted: 0
         SSM reports transmitted: 0
         Leaves transmitted: 0
         Unsuccessful joins recieved count Per Vlan : 0
         Active/Successful joins recieved count Per Vlan: 0
         Active Groups count: 0
         Packets dropped: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |