Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Test SEFOS2

1. Examine the OSPF external routes corresponding to all the NSSA external LSAs.

       SEFOS# show ip ospf route

       OSPF Process Routing Table

       Dest/Mask                     TOS NextHop/Interface Cost Rt.Type   Area
       ---------                     --- -------/--------- ---- -------   ----
       10.2.2.0/255.255.255.0        0   0.0.0.0/vlan2     1    IntraArea 0.0.0.2
       10.4.0.0/255.255.0.0          0   0.0.0.0/vlan1     1    IntraArea 0.0.0.0
       90.1.0.0/255.255.0.0          0   10.2.2.2/vlan2    10   Type2Ext  0.0.0.2
       90.2.0.0/255.255.0.0          0   10.2.2.2/vlan2    10   Type2Ext  0.0.0.2
       90.3.0.0/255.255.0.0          0   10.2.2.2/vlan2    10   Type2Ext  0.0.0.2
       90.4.0.0/255.255.0.0          0   10.2.2.2/vlan2    10   Type2Ext  0.0.0.2
       90.5.0.0/255.255.0.0          0   10.2.2.2/vlan2    10   Type2Ext  0.0.0.2

2. Test the `area default-cost` command.

       SEFOS# configure terminal
       SEFOS(config)# router ospf
       SEFOS(config-router)# area 0.0.0.2 default-cost 50

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |