Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Display a Summary of the Spanning Tree Information for the Configuration

This command displays a summary of port states or the total lines of the STP state section.

- Type.

      SEFOS# show spanning-tree summary

      Spanning Tree port pathcost method is Long
      Spanning tree enabled protocol is MSTP

      MST00 Port Roles and States
      Port-Index  Port-Role    Port-State     Port-Status

      ----------  ---------    ----------     -----------
      1           Designated   Forwarding   Enabled
      2           Disabled     Discarding   Enabled
      3           Disabled     Discarding   Enabled
      4           Disabled     Discarding   Enabled
      5           Disabled     Discarding   Enabled
      6           Disabled     Discarding   Enabled
      7           Disabled     Discarding   Enabled
      8           Disabled     Discarding   Enabled
      9           Disabled     Discarding   Enabled
      10          Disabled     Discarding   Enabled
      11          Disabled     Discarding   Enabled
      12          Disabled     Discarding   Enabled
      13          Disabled     Discarding   Enabled
      14          Disabled     Discarding   Enabled
      15          Disabled     Discarding   Enabled
      16          Disabled     Discarding   Enabled
      17          Disabled     Discarding   Enabled
      18          Disabled     Discarding   Enabled
      19          Disabled     Discarding   Enabled
      20          Disabled     Discarding   Enabled
      21          Disabled     Discarding   Enabled
      22          Disabled     Discarding   Enabled
      23          Disabled     Discarding   Enabled
      24          Disabled     Discarding   Enabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |