Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

### Environmental Specifications

Parameter | Operating Limits
--- | ---
Ambient temperature | 59°F to 89.6°F (15°C to 32°C) Humidity: 10-90% noncondensing
Relative humidity | 20% to 80% noncondensing, 80°F (27°C) maximum wet bulb
Elevation (Sun requirement) | Maximum 10,006 feet (3050 meters) at 77°F (25°C) 2,953 feet (900 meters) at 89.6°F (32°C) Derate maximum ambient 1°C per 300 meters above 900 meters.
Nonoperating Limits | Humidity: 5-95% noncondensing Temperature: -40 to 70°C Altitude: 0-39370 ft (12000 meters)

##### Related Information

- Physical Specifications

- Acoustic Noise Emissions

- Electrical Specifications

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |