Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

### Front Panel Components

No. | Description | Links
--- | --- | ---
1 | NET MGT 0 (Port A) and NET MGT 1, Port B. (from left to right). | Connect the NET MGT Cable Configure Network Management From Web Log Into Oracle ILOM CLI (SER MGT) NET MGT Port
2 | QSFP 10 GbE connectors 1 to 64, four ports each.(from bottom left to right) | QSFP Cables
3 | SER MGT serial management port. | Connect the SER MGT Cable Configure Network Management From CLI (SER MGT) Log Into Oracle ILOM CLI (SER MGT) SER MGT Port
4 | SFP+ ports 65 to 72. (from bottom left to right) | SFP+ Cables

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |