Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuration Guidelines

- GMRP must be disabled for MLD snooping to be enabled.

- To enable fast leave on a port, the port must be connected to a host and not to a switch or hub.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |