Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Display the Pseudo Root ID

- Display the configured pseudo root ID.

  This command displays the port configured as a L2GP only.

      SEFOS# show spanning-tree layer2-gateway-port

      Switch default
      Port Ex0/1
                              PseudoRootId
      Instance      Priority     MacAddress          State
      --------      --------     ----------          ----------
      MST00          4096        00:01:02:03:04:01   Forwarding
      MST01          8192        00:01:02:03:04:02   Forwarding

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |