C H A P T E R 14

SNMPv3

SNMP is the most widely-used network management protocol on TCP/IP-based networks. SNMPv3 is designed mainly to overcome the security shortcomings of SNMPv1 and v2. USM and VACM are the main features added as part of the SNMPv3 specification. USM provides for both encryption and authentication of the SNMP PDUs, while VACM specifies a mechanism for defining access policies for different users with different MIB trees. Also, SNMPv3 specifies a generic management framework, which is expandable for adding new management engines, security models, access control models, and so on. With SNMPv3, the SNMP communication is completely safe and secure.

SNMPv3 is a multi-lingual agent supporting all three versions of SNMP (SNMPv1, SNMPv2c and SNMPv3) while conforming to the latest specifications.

Because SEFOS is started as an agentX-subagent of the Oracle ILOM automatically, some of the commands listed and described specific for SNMP agent in this chapter are not applicable.

Those unsupported commands are noted in this chapter. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of those unsupported commands. Note that only the USM is supported by ILOM.

##

14.1 SNMPv3 Commands

The list of CLI commands for the configuration of SNMPv3 is as follows:

- enable snmpsubagent

- disable snmpsubagent

- show snmp agentx information

- show snmp agentx statistics

- enable snmpagent

- disable snmpagent

- snmp community index

- snmp group

- snmp access

- snmp engineid

- snmp proxy name

- snmp view

- snmp targetaddr

- snmp targetparams

- snmp user

- snmp notify

- snmp-server enable traps snmp authentication

- snmp-server trap udp-port

- snmp-server trap proxy-udp-port

- snmp tcp enable

- snmp trap tcp enable

- snmp-server tcp-port

- snmp-server trap tcp-port

- snmp-server enable traps

- show snmp

- show snmp community

- show snmp group

- show snmp group access

- show snmp engineID

- show snmp viewtree

- show snmp targetaddr

- show snmp targetparam

- show snmp user

- show snmp notif

- show snmp inform statistics

- show snmp-server traps

- show snmp-server proxy-udp-port

- show snmp tcp

### 14.1.1 `enable snmpsubagent`

Enables either snmp agent or agentx-subagent capabilities.

    enable snmpsubagent {master {ip4 ipv4_address} [port number]}

Syntax Description | snmpsubagent - Enables SNMP subagent master - The master agent address. It can be either `ip4` or `ip6`. port - Port number on which master agent listens subagent.
Mode | Global Configuration
Defaults | port - 705
Example | SEFOS(config)# enable snmpsubagent master ip4 10.0.0.5 port 897
Notes | Commands to enable and disable the snmp subagent are used by the SEFOS automatic scripts. Do not use the `enable snmpsubagent` or `disable snmpsubagent` commands from the CLI command interface.

#### Related Commands

- show snmp agentx information - Displays global information of SNMP agentx communications.

- show snmp agentx statistics - Displays all the information regarding SNMP agentx statistics.

### 14.1.2 `disable snmpsubagent`

This command disables agentx-subagent.

    disable snmpsubagent

Mode | Global Configuration
Example | SEFOS(config)# disable snmpsubagent
Notes | Commands to enable and disable the snmp subagent are used by the SEFOS automatic scripts. Do not use the `enable snmpsubagent` or `disable snmpsubagent` commands from the CLI command interface.

#### Related Commands

- show snmp agentx information - Displays global information of SNMP agentx communications.

- show snmp agentx statistics - Displays all the information regarding SNMP agentx statistics.

### 14.1.3 `show snmp agentx information`

Displays global information of SNMP Agentx communications.

    show snmp agentx information

Mode | Priveleged EXEC
Example | SEFOS# show snmp agentx information Agentx Subagent is enabled TransportDomain :TCP Master IP Address :10.0.0.2 Master PortNo :705

### 14.1.4 `show snmp agentx statistics`

Displays all the information regarding SNMP Agentx statistics.

    show snmp agentx statistics

Mode | Global Configuration
Example | SEFOS(config)# show snmp agentx statistics Tx Statistics Transmitted Packets :860 Open PDU :1 Index Allocate PDU :0 Index DeAllocate PDU :0 Register PDU :2 Add Agent Capabilities PDU :0 Notify PDU :0 Ping PDU :20 Remove Agent Capabilities PDU :0 UnRegister PDU :0 Close PDU :0 Response PDU :837 Rx Statistics Rx Packets :859 Get PDU :1 GetNext PDU :836 GetBulk PDU :0 TestSet PDU :0 Commit PDU :0 Cleanup PDU :0 Undo PDU :0 Dropped Packets :0 Parse Drop Errors :1 Open Fail Errors :0 Close PDU :0 Response PDU :21

### 14.1.5 `enable snmpagent`

Enables SNMP agent.

    enable snmpagent

Mode | Global Configuration
Defaults | SNMP agent is enabled.
Example | SEFOS(config)# enable snmpagent

#### Related Commands

- disable snmpagent - Disables SNMP agent.

- enable snmpagent - Enables either snmp agent or agentx-subagent capabilities.

### 14.1.6 `disable snmpagent`

Disables SNMP agent.

    disable snmpagent

Mode | Global Configuration
Example | SEFOS(config)# disable snmpagent

#### Related Commands

- enable snmpagent - Enables SNMP agent.

- enable snmpsubagent - Enables either snmp agent or agentx-subagent capabilities.

### 14.1.7 `snmp community index`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the SNMP community details. The `no` form of the command removes the SNMP community details.

    snmp community index CommunityIndex name CommunityName security SecurityName [context ContextName] [{volatile | nonvolatile}] [transporttag TransportTagIdentifier | none] [contextengineid ContextEngineID]

    no snmp community index CommunityIndex

Syntax Description | CommunityIndex - Community index identifier. CommunityName - Community name. SecurityName - User name. ContextName - Context name through which the management information is accessed when using the community string specified by the corresponding instance of SNMP community name. volatile | nonvolatile - Storage type. TransportTagIdentifier - Transport tag identifier. ContextEngineIdentifier - Context engine identifier.
Mode | Global Configuration
Defaults | Community index - NETMAN/PUBLIC Community name - NETMAN/PUBLIC Security name - None Context name - Null Transport tag - Null Storage type - Volatile
Example | SEFOS(config)# snmp community index myv3com name myv3com security xyz context myinst nonvolatile transporttag myv3tag
Notes | The community index identifier must be unique for every community name entry.

#### Related Commands

- show snmp - Displays the status information of SNMP communications.

- show snmp community - Displays the configured SNMP community details.

### 14.1.8 `snmp group`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures SNMP group details. The `no` form of the command removes the SNMP group details.

    snmp group GroupName user UserName security-model {v1 | v2c | v3} [{volatile | nonvolatile}]

    no snmp group GroupName user UserName security-model {v1 | v2c | v3}

Syntax Description | GroupName - Name of the SNMP group UserName - User name security-model - Security model volatile | nonvolatile - Storage type
Mode | Global Configuration
Defaults | Group name - iso/initial
Example | SEFOS(config)# snmp group myv3group user myv3user security-model v1 volatile

#### Related Commands

- show snmp group - Displays the configured SNMP groups.

- show snmp user - Displays the configured SNMP users.

### 14.1.9 `snmp access`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the SNMP group access details. The `no` form of the command removes the SNMP group access details.

    snmp access GroupName {v1 | v2c | v3 {auth | noauth | priv}} [read ReadView | none] [write WriteView | none] [notify NotifyView | none] [{volatile | nonvolatile}] [context ContextName]

    no snmp access GroupName {v1 | v2c | v3 {auth | noauth | priv}} [context ContextName]

Syntax Description | GroupName - Name of the group. v1 | v2c | v3 - Version of the SNMP. auth - Enables authentication: MD5 or SHA packet authentication. noauth - Disables authentication. priv - Specifies both authentication and privacy. read - A read view identifier. write - A write view identifier. notify - A notification view identifier. volatile | nonvolatile - Storage type. ContextName - Name of the SNMP context.
Mode | Global Configuration
Defaults | Group name - iso Read/write/notify view - iso Storage type - volatile Group name - initial Read/write/notify view - restricted Storage type - non-volatile Group name - initial Read/write/notify view - iso Storage type - non-volatile
Example | SEFOS(config)# snmp access myv2group v2 read v2readview write v2writeview notify v2notifyview nonvolatile
Notes | To configure an SNMP access along with the group, a group must have already been created using the `snmp group` command. Version 3 is the most secure model as it allows packet encryption with the `priv` key word.

#### Related Commands

- snmp group - Configures SNMP group details.

- snmp view - Configures the SNMP view.

- show snmp group - Displays the configured SNMP groups.

- show snmp group access - Displays the configured SNMP group access. details.

- show snmp viewtree - Displays the configured SNMP tree views.

### 14.1.10 `snmp engineid`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the engine identifier. The `no` form of the command removes the configured engine identifier.

    snmp engineid EngineIdentifier

    no snmp engine-id

Syntax Description | EngineIdentifier - Engine identifier.
Mode | Global Configuration
Defaults | 80.00.08.1c.04.46.53
Example | SEFOS(config)# snmp engineid 80.0.08.1c.04.5f.a9
Notes | The Engine ID must be given as octets in hexadecimal separated by dots and the allowed length is 5 to 32 octets. SNMP engine ID is an administratively unique identifier. Changing the value of the SNMP engine ID has significant effects. All the user information will be updated automatically to reflect the change

#### Related Commands

- snmp engineid - Displays the engine identifier.

- show snmp user - Displays the configured SNMP users.

### 14.1.11 `snmp proxy name`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the proxy. The no form of the command removes the proxy.

    snmp proxy name ProxyName ProxyType {Read | Write | inform | Trap} ContextEngineID EngineId TargetParamsIn TargetParam TargetOut TargetOut [ContextName ProxyContextName] [StorageType {volatile | nonvolatile}]

    no snmp proxy name ProxyName

Syntax Description | ProxyName - The locally arbitrary, but unique identifier associated with the `tProxyEntry`. This will be the index used for the proxy table. ProxyType - Type of message that are forwarded using the translation parameters. Options are: Read Write Inform Trap ContextEngineID - Context engine identifier contained in messages that are forwarded using the translation parameters. TargetParamsIn - This object selects an entry in the `snmpTargetParamsTable`. The selected entry is used to determine which row of the `snmpProxyTable` is to be used for forwarding the received messages. TargetOut - This object selects a management target defined in the `snmpTargetAddrTable` (in the SNMP-TARGET-MIB). The selected target is defined by an entry in the `snmpTargetAddrTable` whose index value (`snmpTargetAddrName`) is equal to this object. This object is only used when selection of a single target is required. That is, when forwarding an incoming read or write request. ContextName - Context name contained in messages that are forwarded using the translation parameters. StorageType - Storage type. Options are: volatile nonvolatile
Mode | Global Configuration
Defaults | Storage Type - nonvolatile
Example | SEFOS(config)# snmp proxy name proxy1 ProxyType write ContextEngineID 80.00.08.1c.04.46.53 TargetParamsIn param2 TargetOut target2 ContextName pxyctxtname StorageType nonvolatile

### 14.1.12 `snmp view`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the SNMP view. The `no` form of the command removes the SNMP view.

    snmp view ViewName OIDTree [mask OIDMask] {included | excluded} [{volatile | nonvolatile}]

    no snmp view ViewName OIDTree

Syntax Description | ViewName - View name OIDTree - Object identifier OIDMask | none - Defines views’ subtrees included | excluded - Type of view volatile | nonvolatile - Type of storage
Mode | Global Configuration
Defaults | View Name - iso/restricted OIDTree - 1 OIDMask - None View type - included Storage type - non-volatile
Example | SEFOS(config)# snmp view v2readview 1.3.6.1 mask 1.1.1.1 included nonvolatile
Notes | To configure an SNMP view (read/write/notify), a group must have already been created using the snmp group command and SNMP group access must be configured using the snmp access command.

#### Related Commands

- snmp access - Configures the SNMP group access details.

- show snmp viewtree - Displays the configured SNMP tree views.

- show snmp group access - Displays the configured SNMP group access details.

### 14.1.13 `snmp targetaddr`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the SNMP target address. The `no` form of the command removes the configured SNMP target address.

    snmp targetaddr TargetAddressName param ParamName {IPAddress | IP6Address} [timeout Seconds(1-1500)] [retries RetryCount(1-3)] [taglist TagIdentifier | none] [{volatile | nonvolatile}]

    no snmp targetaddr TargetAddressName

Syntax Description | TargetAddressName - Name of the target address (host). param - SNMP parameter name. IPAddress | IP6Address - IP/IP6 Address of the host. timeout - The time the SNMP agent waits for a response from the SNMP manager before retransmitting the inform request message. retries - The maximum number of times the agent can retransmit the inform request message. taglist - Tag identifier. volatile | nonvolatile - Storage type.
Mode | Global Configuration
Defaults | ParamName - Internet IPAddress - 10.0.0.10 taglist - snmp Storage type - volatile
Example | SEFOS(config)# snmp targetaddr sefosmgr param sefosd 10.0.0.10 taglist mytag nonvolatile
Notes | Target param must have been configured.

#### Related Commands

- show snmp targetaddr - Displays the configured SNMP target addresses.

- snmp targetparams - Configures the SNMP target parameters.

- show snmp targetparam - Displays the configured SNMP target address parameters.

### 14.1.14 `snmp targetparams`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the SNMP target parameters. The `no` form of the command removes the SNMP target parameters.

    snmp targetparams ParamName user UserName security-model {v1 | v2c | v3 {auth | noauth | priv}} message-processing {v1 | v2c | v3} [{volatile | nonvolatile}]

    no snmp targetparams ParamName

Syntax Description | ParamName - SNMP parameter name. user - User name. security-model - Security model. auth - Enables authentication: MD5 or SHA packet authentication. noauth - Disables authentication. priv - Specifies both authentication and privacy. message-processing - Message processing model. volatile | nonvolatile - Storage type.
Mode | Global Configuration
Defaults | ParamName - Internet User/Security Name - None Security Model - v2c Security Level - NoauthNoPriv Message Processing Model - v2c Storage Type - Non-volatile ParamName - test1 User/Security Name - None Security Model - v1 Security Level - NoauthNoPriv Message Processing Model - v1 Storage Type - Non-volatile
Example | SEFOS(config)# snmp targetparams param1 user user1 security-model v3 noauth message-processing v3
Notes | User information must have been configured prior to the configuration of SNMP target parameters.

#### Related Commands

- snmp user - Configures the SNMP user details.

- show snmp targetparam - Displays the configured SNMP target address parameters.

- show snmp user - Displays the configured SNMP users.

### 14.1.15 `snmp user`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the SNMP user details. The `no` form of the command removes the SNMP user details.

    snmp user UserName [auth {md5 | sha} passwd [priv DES passwd]] [{volatile | nonvolatile}]

    no snmp user UserName

Syntax Description | UserName - Name of the user. auth - Authentication algorithm. Can be MD5 or SHA. passwd - Password associated with the authentication type. priv DES - Private encryption password volatile | nonvolatile - Storage type. Cann be either volatile or non-volatile.
Mode | Global Configuration
Defaults | UserName - Initial Authentication Protocol - None Privacy Protocol - None Storage type - Non-volatile Storage type - Non-volatile
Example | SEFOS(config)# snmp user user1
Notes | SNMP passwords are localized using the local SNMP engine ID.

#### Related Commands

- show snmp engineID - Displays the engine identifier.

- show snmp user - Displays the configured SNMP users.

### 14.1.16 `snmp notify`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the SNMP notification details. The `no` form of this command removes the SNMP notification details.

    snmp notify NotifyName tag TagName type {Trap | Inform} [{volatile | nonvolatile}]

    no snmp notify NotifyName

Syntax Description | NotifyName - Notification Name tag - Tag Name type - Type of Notification volatile | nonvolatile - Storage type of the notification details
Mode | Global Configuration
Defaults | Notify Name - sefos/sefos1 Notify Tag - sefos/sefos1 Storage type - volatile
Example | SEFOS(config)# snmp notify note1 tag tag1 type Inform

#### Related Commands

- show snmp notif - Displays the configured SNMP notifications.

- show snmp targetaddr - Displays the configured SNMP target addresses.

### 14.1.17 `snmp-server enable traps snmp authentication`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command enables generation of authentication traps for SNMPv1 and SNMPv2c. The `no` form of the command disables generation of authentication traps for SNMPv1 and SNMPv2c.

    snmp-server enable traps snmp authentication

    no snmp-server enable traps snmp authentication

Mode | Global Configuration
Defaults | Generation of authentication traps is disabled by default.
Example | SEFOS(config)# snmp-server enable traps snmp authentication

### 14.1.18 `snmp-server trap udp-port`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the udp port over which agent sends the trap. The `no` form of the command configures the snmp agent to sent trap on default udp port.

    snmp-server trap udp-port port

    no snmp-server trap udp-port

Syntax Description | port - Port number.
Mode | Global Configuration
Example | SEFOS(config)# snmp-server trap udp-port 1234

#### Related Commands

- show snmp notif - Displays the configured SNMP notification types.

### 14.1.19 `snmp-server trap proxy-udp-port`

Configures the udp port over which agent sends the trap. The `no` form of the command configures the snmp agent to sent trap on default udp port.

    snmp-server trap proxy-udp-port port

    no snmp-server trap proxy-udp-port

Syntax Description | port - Port number.
Mode | Global Configuration
Defaults | 162
Example | SEFOS(config)# snmp-server trap proxy-udp-port 162

#### Related Commands

- show snmp-server proxy-udp-port - Displays the proxy udp port.

### 14.1.20 `snmp tcp enable`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command enables sending snmp messages over tcp. The `no` form of the command disables sending snmp messages over tcp.

    snmp tcp enable

    no snmp tcp enable

Mode | Global Configuration
Defaults | Disabled.
Example | SEFOS(config)# snmp tcp enable

#### Related Commands

- show snmp tcp - Displays the configuration for snmp over tcp.

### 14.1.21 `snmp trap tcp enable`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command enables sending snmp trap messages over tcp. The `no` form of the command disables sending snmp trap messages over tcp.

    snmp trap tcp enable

    no snmp trap tcp enable

Mode | Global Configuration
Defaults | Disabled.
Example | SEFOS(config)# snmp trap tcp enable

#### Related Commands

- show snmp tcp - Displays the configuration for snmp over tcp.

### 14.1.22 `snmp-server tcp-port`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the tcp port over which agent sends the snmp message. The `no` form of the command configures the snmp agent to sent snmp message on default tcp port.

    snmp-server tcp-port port

    no snmp-server tcp-port

Syntax Description | port - Port number.
Mode | Global Configuration
Defaults | 161
Example | SEFOS(config)# snmp-server tcp-port 161

#### Related Commands

- show snmp tcp - Displays the configuration for snmp over tcp.

### 14.1.23 `snmp-server trap tcp-port`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command configures the tcp port over which agent sends the trap. The `no` form of the command configures the snmp agent to sent trap on default tcp port.

    snmp-server trap tcp-port port

    no snmp-server trap tcp-port

Syntax Description | port - Port number.
Mode | Global Configuration
Defaults | 162
Example | SEFOS(config)# snmp-server trap tcp-port 162

#### Related Commands

- show snmp tcp - Displays the configuration for snmp over tcp.

### 14.1.24 `snmp-server enable traps`

Enables generation of a particular trap. The `no` form of the command disables generation of a particular trap.

    snmp-server enable traps {[firewall-limit] [linkup] [linkdown] [coldstart]}

    no snmp-server enable traps {[firewall-limit] [linkup] [linkdown]  [coldstart]}

Syntax Description | firewall-limit - Firewall attack summary trap. linkup - Linkup trap. linkdown - Linkdown trap. coldstart - Coldstart trap.
Mode | Global Configuration
Notes | Do not use this command for trapping the link status. Link up (`linkup`) and link down (`linkdown`) are specific to a particular interface, so you must be in that interface mode to enable and disable the link status. Instead, use the following commands: `snmp trap link-status` to enable the link up and down events. `no snmp trap link-status` to disable the link up and down events. For example: `SEFOS(config)#` int ex 0/1 `SEFOS(config-if)#` snmp trap link-status

#### Related Commands

- show snmp-server traps - Displays the set of traps that are currently enabled.

### 14.1.25 `show snmp`

Displays the status information of SNMP communications.

    show snmp

Mode | Privileged EXEC
Example | SEFOS# show snmp 0 SNMP Packets Input 0 Bad SNMP Version errors 0 Unknown community name 0 Get request PDUs 0 Get Next PDUs 0 Set request PDUs 0 SNMP Packets Output 0 Too big errors 0 No such name errors 0 Bad value errors 0 General errors 0 Trap PDUs
| 0 SNMP Rollback failures SNMP Manager-role output packets 0 Drops SNMP Informs: 0 Inform Requests generated 0 Inform Responses received 0 Inform messages Dropped 0 Inform Requests awaiting Acknowledgement SNMP Trap Listen Port is 162

### 14.1.26 `show snmp community`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the configured SNMP community details.

    show snmp community

Mode | Privileged EXEC
Example | SEFOS# show snmp community Community Index: NETMAN Community Name: NETMAN Security Name: none Context Name: Transport Tag: Storage Type: volatile Row Status: active ------------------------------ Community Index: PUBLIC Community Name: PUBLIC Security Name: none Context Name: Transport Tag: Storage Type: volatile Row Status: active

#### Related Commands

- snmp community index - Configures the SNMP community details.

### 14.1.27 `show snmp group`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the configured SNMP groups.

    show snmp group

Mode | Privileged EXEC
Example | SEFOS# show snmp group Security Model: v1 Security Name: none Group Name: iso Storage Type: volatile Row Status: active ------------------------------ Security Model: v2c Security Name: none Group Name: iso Storage Type: volatile Row Status: active ------------------------------ Security Model: v3 Security Name: initial Group Name: initial Storage Type: nonVolatile Row Status: active ------------------------------ Security Model: v3 Security Name: templateMD5 Group Name: initial Storage Type: nonVolatile Row Status: active ------------------------------ Security Model: v3 Security Name: templateSHA Group Name: initial Storage Type: nonVolatile Row Status: active
Notes |

#### Related Commands

- snmp group - Configures the SNMP group details.

- snmp user - Configures the SNMP user details.

### 14.1.28 `show snmp group access`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the configured SNMP group access details.

    show snmp group access

Mode | Privileged EXEC
Example | SEFOS# show snmp group access Group Name: iso Read View: iso Write View: iso Notify View: iso Storage Type: volatile Row Status: active ------------------------------ Group Name: iso Read View: iso Write View: iso Notify View: iso Storage Type: volatile Row Status: active ------------------------------ Group Name: initial Read View: restricted Write View: restricted Notify View: restricted Storage Type: nonVolatile Row Status: active ------------------------------ Group Name: initial Read View: iso Write View: iso Notify View: iso Storage Type: nonVolatile Row Status: active

#### Related Commands

- snmp access - Configures the SNMP group access details

- snmp view - Configures the SNMP view

### 14.1.29 `show snmp engineID`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the engine identifier.

    show snmp engineID

Mode | Privileged EXEC
Example | SEFOS# show snmp engineID EngineId: 80.00.08.1c.04.46.53

#### Related Commands

- snmp engineid - Configures the engine identifier.

### 14.1.30 `show snmp viewtree`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the configured SNMP tree views.

    show snmp viewtree

Mode | Privileged EXEC
Example | SEFOS# show snmp viewtree View Name: iso Subtree OID: 1 Subtree Mask: View Type: included Storage Type: nonVolatile Row Status: active ------------------------------ View Name: restricted Subtree OID: 1 Subtree Mask: View Type: included Storage Type: nonVolatile Row Status: active ------------------------------

#### Related Commands

- snmp view - Configures the SNMP view.

### 14.1.31 `show snmp targetaddr`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the configured SNMP target addresses.

    show snmp targetaddr

Mode | Privileged EXEC
Example | SEFOS# show snmp targetaddr Target Address Name: sefosmanager IP Address: 10.0.0.10 Tag List: snmp Parameters: internet Storage Type: volatile Row Status: active ------------------------------

#### Related Commands

- snmp targetaddr - Configures the SNMP target address.

- snmp targetparams - Configures the SNMP target parameters.

- snmp notify - Configures the SNMP notification details.

### 14.1.32 `show snmp targetparam`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the configured SNMP target address parameters.

    show snmp targetparam

Mode | Privileged EXEC
Example | SEFOS# show snmp targetparam Target Parameter Name: internet Message Processing Model: v2c Security Model: v2c Security Name: none Security Level: noAuthNoPriv Storage Type: volatile Row Status: active ------------------------------ Target Parameter Name: test1 Message Processing Model: v1 Security Model: v1 Security Name: none Security Level: noAuthNoPriv Storage Type: volatile Row Status: active

#### Related Commands

- snmp targetparams - Configures the SNMP target parameters.

- snmp user - Configures the SNMP user details.

### 14.1.33 `show snmp user`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the configured SNMP users.

    show snmp user

Mode | Privileged EXEC
Example | SEFOS# show snmp user Engine ID: 80.00.08.1c.04.46.53 User: initial Authentication Protocol: none Privacy Protocol: none Storage Type: nonVolatile Row Status: active ------------------------------ Engine ID: 80.00.08.1c.04.46.53 User: templateMD5 Authentication Protocol: MD5 Privacy Protocol: none Storage Type: nonVolatile Row Status: active ------------------------------ Engine ID: 80.00.08.1c.04.46.53 User: templateSHA Authentication Protocol: SHA Privacy Protocol: DES_CBC Storage Type: nonVolatile Row Status: active ------------------------------

#### Related Commands

- snmp user - Configures the SNMP user details.

- show snmp community - Displays the configured SNMP community details.

### 14.1.34 `show snmp notif`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the configured SNMP notification types.

    show snmp notif

Mode | Privileged EXEC
Example | SEFOS# show snmp notif Notify Name: sefos Notify Tag: sefos Notify Type: trap Storage Type: volatile Row Status: active ------------------------------ Notify Name: sefos1 Notify Tag: sefos1 Notify Type: trap Storage Type: volatile Row Status: active

#### Related Commands

- snmp notify - Configures the SNMP notification details.

- snmp targetparams - Configures the SNMP target parameters.

### 14.1.35 `show snmp inform statistics`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the inform message statistics.

    show snmp inform statistics

Mode | Privileged EXEC
Example | SEFOS# show snmp inform statistics Target Address Name : sefosmanager IP Address : 10.0.0.10 Inform messages sent : 20 Acknowledgement awaited for : 2 Inform messages Inform messages dropped : 0 Acknowledgement failed for : 0 Inform messages Informs retransmitted: 0 Inform responses received: 18

### 14.1.36 `show snmp-server traps`

This command displays the set of traps that are currently enabled.

    show snmp-server traps

Mode | Privileged EXEC
Example | SEFOS# show snmp-server traps Currently enabled traps: ------------------------ linkup,linkdown,

#### Related Commands

- snmp-server enable traps - Enables generation of a particular trap.

### 14.1.37 `show snmp-server proxy-udp-port`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the proxy udp port.

    show snmp-server proxy-udp-port

Mode | Privileged EXEC
Example | SEFOS# show snmp-server proxy-udp-port snmp-server proxy-udp-port : 162

#### Related Commands

- snmp-server trap proxy-udp-port - Configures the udp port over which agent sends the trap.

### 14.1.38 `show snmp tcp`

Note - This command is not currently supported. Refer to the Oracle Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide for the ILOM equivalent of this command.

This command displays the configuration for snmp over tcp.

    show snmp tcp

Mode | Privileged EXEC
Example | SEFOS# show snmp tcp snmp over tcp disabled snmp trap over tcp disabled snmp listen tcp port 161 Snmp listen tcp trap port 162

#### Related Commands

- snmp tcp enable - Enables sending snmp messages over tcp.

- snmp trap tcp enable - Enables sending snmp trap messages over tcp.

- snmp-server tcp-port - Configures the tcp port over which agent sends the snmp message.

- snmp-server trap tcp-port - Configures the tcp port over which agent sends the trap.

Copyright © 2012, Oracle and/or its affiliates. All rights reserved.